[55B] AUTOMATIC AIR CONDITIONER - - CONDENSER AND CONDENSER FAN MOTOR - REMOVAL AND INSTALLATION <2000- DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <2000- DOHC>
Pre-removal and Post-installation Operation Refrigerant Draining and Refilling (Refer to GROUP 55A, On vehicle service ). Air Cleaner Removal and Installation (Refer to GROUP 15, Air Cleaner ). Condense Tank and Support Upper Insulator Removal and Installation (Refer to GROUP 14, Radiator ).
|  |  | Fan shroud assembly removal steps
--- | --- | --- | ---
<<A>> |  | 1. | Fan shroud assembly
|  | 2. | Fan
|  | 3. | Fan motor
|  | 4. | Fan shroud
|  |  | Condenser removal steps
<<B>> |  | 5. | Flexible discharge hose connection
<<B>> |  | 6. | Liquid pipe A connection
|  | 7. | O ring
| >>A<< | 8. | Condenser assembly
|  | 9. | Clamp
|  | 10. | Receiver
|  | 11. | O ring
|  | 12. | Condenser
|  |  | Air guide panel removal steps
|  | • | Front bumper (Refer to GROUP 51, Front bumper ).
|  | 13. | Air guide panel
| REMOVAL SERVICE POINT
| <<A>> CONDENSER FAN SHROUD ASSEMBLY REMOVAL
| Remove the two upper radiator fan shroud bolts. Reaching through the gap between the radiator and the radiator fan shroud, release the clip shown.
| <<B>> FLEXIBLE SUCTION HOSE AND LIQUID PIPE A DISCONNECTION CAUTION As the compressor oil and receiver are highly moisture absorbent, use a non-porous material to plug the hose and nipples. To prevent the entry of dust or other foreign bodies, plug the dismantled hose and condenser assembly nipples.
| INSTALLATION SERVICE POINT
| >>A<< CONDENSER INSTALLATION When replacing the condenser, refill it with a specified amount of compressor oil and install it. (to the vehicle). Compressor oil: SUN PAG 56 Quantity: 15 mL

[55B] AUTOMATIC AIR CONDITIONER - - CONDENSER AND CONDENSER FAN MOTOR - REMOVAL AND INSTALLATION <2000- DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation