[42] BODY - - SUNROOF | PRINT PAGE / INDEX / PRIOR / NEXT

SUNROOF
Some models come with a power sliding glass sunroof with a tilt up mechanism <Except vehicles for Hong Kong spec>. As an optional equipment for some models, the electrical sliding glass sunroof with the tilt-up mechanism is available in front, and the fixed-type roof window glass is available in rear <Vehicles for Hong Kong spec>. This sunroof features the following characteristics. The sunroof tilts up approximately 30 mm to improve ventilation. The sunroof features an outer slider mechanism and enhances head clearance in the front and back seat to improve riding comfort. The integrated switch allows for all slide open/close, tilt up/down and stop operations. All operations are available at one touch. If external force is applied during slide closing or tilt down operations that obstructs operations, then the roof lid glass will reverse and stop according to the jam prevention mechanism. The system features a function to open approximately 30 mm every time the close/tilt down switch is pressed, until the sunroof is fully open, by canceling the jam prevention mechanism. The sunroof timer function is adopted <Except vehicles for Argentina>. As an adjustment function for the keyless entry system, the fully closing operation of the sunroof can be switched on/off by the lock button on the transmitter <Vehicles for Hong Kong spec> (GROUP 54B, SMART WIRING SYSTEM ). The fixed roof window glass at rear can let plenty of light into the passenger compartment and increase open airy feeling <Vehicles for Hong Kong spec>.
CONSTRUCTION DIAGRAM
DESCRIPTION OF STRUCTURE AND OPERATION
Sunroof timer function The sunroof has a timer function which allows the roof lid glass to be closed or opened after the ignition switch is turned OFF (Refer to GROUP 54B, SMART WIRING SYSTEM ). During the timer operation, if the driver's door is opened, the time is extended by 30 seconds from the moment. However, the timer is expired when the driver's door is closed during the extended time <Except vehicles for Australia, New Zealand (2400) and Argentina>. During the timer operation, if the driver's door or front passenger's door is opened, the timer is expired at the moment <Vehicles for Australia and New Zealand (2400)>.
| MOTOR
| There is s motor assembled on the rear-side of the housing and the structure consists of the motor unit, drive gear and sunroof ECU.
Sunroof-ECU The sunroof ECU incorporates a microcomputer and controls the motor operations according to the sunroof switch signal and ETACS signal state.

[42] BODY - - SUNROOF | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation