[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - MUT-III | PRINT PAGE / INDEX / PRIOR / NEXT

| MUT-III Refer to the "MUT-III OPERATING INSTRUCTIONS" for instructions on handling the MUT-III.
| Connect the MUT-III to the diagnosis connector as shown in the illustration. CAUTION Turn the ignition switch to the LOCK (OFF) position before connecting or disconnecting the MUT-III.

[0] GENERAL - - PRECAUTIONS BEFORE SERVICE - MUT-III | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation