[14] ENGINE COOLING - - WATER PUMP - REMOVAL AND INSTALLATION <4G69-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

REMOVAL AND INSTALLATION <4G69-SOHC>
Pre-removal Operation Engine Coolant Draining (Refer to ). Timing Belt Removal (Refer to GROUP 11E, Timing Belt ). | Post-installation Operation Timing Belt Installation (Refer to GROUP 11E, Timing Belt ). Engine Coolant Refilling (Refer to ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Water pump
|  | 2. | Water pump gasket
| >>A<< | 3. | O-ring
| INSTALLATION SERVICE POINT
| >>A<< O-RING INSTALLATION
| Fit the O-ring to the groove in the water inlet pipe. Then lubricate the O-ring and the inside of the water pump with water, and then insert the pipe to the water pump.

[14] ENGINE COOLING - - WATER PUMP - REMOVAL AND INSTALLATION <4G69-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation