[55B] AUTOMATIC AIR CONDITIONER - - ON-VEHICLE SERVICE - IDLE-UP OPERATION CHECK <2000-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| IDLE-UP OPERATION CHECK <2000-DOHC> Before inspection and adjustment, set vehicle in the following condition: Engine coolant temperature: 80 - 90 °C Lights, electric cooling fan and accessories: Set to OFF Transmission: Neutral ("N" or "P" for vehicles with A/T) Steering wheel: Straightforward Check whether or not the idle speed is the standard value. Refer to GROUP 11C, On-vehicle Service - Idle Speed Check . Standard value: 750 ± 100 r/min When the A/C is running after turning the A/C switch to ON, and the blower switch to the 3(MH) or 4(HI) position, check to be sure that the idle-up speed is at the standard value. Standard value SOHC: 850 ± 100 r/min DOHC: 800 ± 100 r/min NOTE: It is not necessary to make an adjustment, because the idling speed is automatically adjusted by the ISC system. If, however, a deviation from the standard value occurs for some reason, check the ISC system.

[55B] AUTOMATIC AIR CONDITIONER - - ON-VEHICLE SERVICE - IDLE-UP OPERATION CHECK <2000-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation