[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW RELAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| POWER WINDOW RELAY CHECK
BATTERY VOLTAGE | TESTER CONNECTION | SPECIFIED CONDITION
--- | --- | ---
Not applied | 4 - 5 | Open circuit
Connect terminal No. 1 and the positive battery terminal. Connect terminal No. 3 and the negative battery terminal. | Less than 2 ohms

[42] BODY - - DOOR - ON-VEHICLE SERVICE - POWER WINDOW RELAY CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation