[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - Inspection procedure P-20: The hood switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection procedure P-20: The hood switch signal is not received.
| CAUTION Whenever the ECU is replaced, ensure that the input signal circuit is normal.
| COMMENTS ON TROUBLE SYMPTOM Input signal from the hood switch is used to operate the security alarm function. If the signal is abnormal, the security alarm function will not work normally.
| POSSIBLE CAUSES Malfunction of the hood switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Connector check: A-33 hood switch connector Q: Is the check result normal? YES: Go to Step 2. NO: Repair the connector.
| Step 2. Check the hood switch. Refer to GROUP 42 - Hood . Q: Is the check result normal? YES: Go to Step 3. NO: Replace the hood switch.
| Step 3. Measure the resistance at the A-33 hood switch connector. Disconnect the connector, and measure at the wiring harness side. Continuity between A-33 hood switch connector terminal No.2 and body earth OK: 2Ω or less Q: Is the check result normal? YES: Go to Step 5. NO: Go to Step 4.
| Step 4. Check the wiring harness between A-33 hood switch connector terminal No.2 and body earth. Check the earth wires for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 5. Connector check: C-220 ETACS-ECU connector Q: Is the check result normal? YES: Go to Step 6. NO: Repair the connector.
| Step 6. Check the wiring harness between C-220 ETACS-ECU connector terminal No.21 and A-33 hood switch connector terminal No.1. NOTE: Prior to the wiring harness inspection, check intermediate connector C-116, and repair if necessary. Check the input line for open circuit. Q: Is the check result normal? YES: Go to Step 7. NO: Repair the wiring harness.
| Step 7. Retest the system. Check that the hood switch signal is received normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - INPUT SIGNAL PROCEDURES - Inspection procedure P-20: The hood switch signal is not received. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation