[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 3: When the Auto-cruise Control "CANCEL" Switch is Set to ON, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

Inspection Procedure 3: When the Auto-cruise Control "CANCEL" Switch is Set to ON, Auto-cruise Control is not Cancelled.
COMMENTS ON TROUBLE SYMPTOM The cause is probably an open-circuit in the circuit inside the auto-cruise control CANCEL switch.
PROBABLE CAUSE Malfunction of the auto-cruise control switch.
DIAGNOSIS Replace the auto-cruise control switch (Refer to ). Then check the malfunction is eliminated.

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - SYMPTOM PROCEDURES - Inspection Procedure 3: When the Auto-cruise Control "CANCEL" Switch is Set to ON, Auto-cruise Control is not Cancelled. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation