[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - TRANSFER - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

TRANSFER

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Dust seal guard
| >>E<< | 2. | Oil seal
| >>D<< | 3. | Oil seal
| >>A<< | 4. | O-ring
| >>A<< | 5. | O-ring
| >>C<< | 6. | Oil seal
| >>B<< | 7. | Oil seal
| >>A<< | 8. | O-ring
|  | 9. | Transfer cover
|  | 10. | Transfer
| REASSEMBLY SERVICE POINTS
| >>A<< O-RING INSTALLATION Coat the O-rings with gear oil before installation.
| >>B<< OIL SEAL INSTALLATION
| Use the special tool Oil seal installer (MD998800) to install the oil seal.
| >>C<< OIL SEAL INSTALLATION
| Use the special tools to install the oil seal. Installer adapter (MB990934) Handle (MB990938)
| >>D<< OIL SEAL INSTALLATION
| CAUTION Install the oil seal after applying ATF to its lip. Use the special tools to install the oil seal. Arm bushing remover and installer ring (MB990887) Bushing remover and installer base (MB990891)
| >>E<< OIL SEAL INSTALLATION
| CAUTION Install the oil seal after applying gear oil to its lip. Use the special tool Installer adapter (MB990936) to install the oil seal.

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - TRANSFER - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation