[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ON-VEHICLE SERVICE - ON-VEHICLE SERVICE | PRINT PAGE / INDEX / PRIOR / NEXT

ON-VEHICLE SERVICE

| ON-VEHICLE SERVICE
| THROTTLE BODY (THROTTLE VALVE AREA) CLEANING Remove the air intake hose from the throttle body. Spray cleaning fluid on a clean cloth. CAUTION Do not spray the cleaning fluid directly to the throttle valve. Make sure the cleaning fluid does not enter the motor from the bypass line. Also make sure it does not enter the sensor through the shaft. Be careful not to rub off the molybden applied around the throttle valve shaft.
| Wipe off the dirt around the throttle valve with the cloth sprayed with cleaning fluid. Attach the air intake hose. Adjust the basic idle speed (Refer to ).

[13B] MULTIPORT FUEL INJECTION (MPI) <4G64> - - ON-VEHICLE SERVICE - ON-VEHICLE SERVICE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation