[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - IDLE-UP OPERATION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| IDLE-UP OPERATION CHECK Before inspection and adjustment, set vehicle in the following condition: Engine coolant temperature: 80 - 90 °C Lamps, electric cooling fan and accessories: Set to OFF Transmission: Neutral ("N" or "P" for vehicles with A/T) Steering wheel: Straightforward Check whether or not the idle speed is the standard value. Refer to GROUP 11A, On-vehicle Service - IDLE SPEED CHECK . <2000> Refer to GROUP 11A, On-vehicle Service - IDLE SPEED AND IDLE MIXTURE CHECK AND AJUSTMENT . <2400-except MIVEC> Refer to GROUP 11E, On-vehicle Service - IDLE SPEED CHECK . <2400-MIVEC> Standard value: 700 ± 100 r/min When the A/C is running after turning the A/C switch to ON, and the blower switch to the 3(MH) or 4(HI) position, check to be sure that the idle speed is at the standard value. Standard value: 850 ± 100 r/min NOTE: It is not necessary to make an adjustment, because the idling speed is automatically adjusted by the ISC system. If, however, a deviation from the standard value occurs for some reason, check the ISC system.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - IDLE-UP OPERATION CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation