[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - SIMPLE INSPECTION OF THE A/C PRESSURE SENSOR | PRINT PAGE / INDEX / PRIOR / NEXT

| SIMPLE INSPECTION OF THE A/C PRESSURE SENSOR Assemble a manifold gauge onto the high pressure service valve. Turn ON the engine and then turn ON the air conditioner switch.
| Check to see that the voltage between the A/C pressure sensor terminal No.2 and body earth reflects the specifications of the Figure. NOTE: The allowance shall be defined as ± five percents.

[55A] HEATER, AIR CONDITIONER AND VENTILATION - - ON-VEHICLE SERVICE - SIMPLE INSPECTION OF THE A/C PRESSURE SENSOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation