[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - INDIVIDUAL COMPONENT SERVICE | PRINT PAGE / INDEX / PRIOR / NEXT

INDIVIDUAL COMPONENT SERVICE WARNING If heat damage may occur during paint work, remove the SRS-ECU, the air bag modules, the clock spring, front seats, and the seat belt with pre-tensioner. SRS-ECU, air bag module, clock spring and impact sensor: 93° C or more Seat belt with pre-tensioner: 90°C or more If the SRS components are removed for the purpose of check, sheet metal repair, painting, etc., they should be stored in a clean, dry place until they are reinstalled. If the SRS components are to be removed or replaced as a result of maintenance, troubleshooting etc., follow the service procedures that follow. (Front impact sensor; refer to , SRS-ECU; refer to , Air bag modules and clock spring; refer to , Side impact sensor; refer to , Seat belt with pre-tensioner; refer to ).

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - INDIVIDUAL COMPONENT SERVICE | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation