[11A] ENGINE MECHANICAL <4G6-SOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION The 4G63-SOHC engine and 4G64-SOHC engine have been adopted in the new OUTLANDER. These engines are basically the same as that of the 4G6-SOHC engine of the previous GALANT.
MAJOR SPECIFICATIONS
Items | 4G63-SOHC | 4G64-SOHC
--- | --- | ---
Total displacement mL | 1,997 | 2,351
Combustion chamber | Pent roof type
Bore × Stroke mm | 85.0 × 88.0 | 88.5 × 100.0
Compression ratio | 9.5 | 9.0
Camshaft-valve arrangement | SOHC-16valves
Valve timing | Intake opening | BTDC 11° | BTDC 16°
Intake closing | ABDC 53° | ABDC 53°
Exhaust opening | BBDC 63° | BBDC 50°
Exhaust closing | ATDC 21° | ATDC 16°
Maximum output | EEC-NET kW/r·min | 93/5,500 | 100/5,000
SAE-GROSS HP/r·min | 125/5,500 | 134/5,000
Maximum torque | EEC-NET N·m/r·min | 173/4,500 | 200/2,500
SAE-GROSS kgf·m/r·min | 17.6/4,500 | 20.4/2,500
Lash adjuster | Equipped

[11A] ENGINE MECHANICAL <4G6-SOHC> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation