[3] WELDED PANEL REPLACEMENT - - FRONT DOOR OUTER PANEL | PRINT PAGE / INDEX / PRIOR / NEXT

FRONT DOOR OUTER PANEL Adhesive : Urethane body sealer Brand : 3M ATD Part No.8542 or equivalent NOTE: After hemming the front door outer panel, MIG spot weld the flange overlap section at a pitch of 50 mm.
NOTE ON REPAIR WORK
REMOVAL Since it is difficult to replace the sash due to a pressed door structure, cut the outer panel from the bottom of the sash.

[3] WELDED PANEL REPLACEMENT - - FRONT DOOR OUTER PANEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation