[11E] ENGINE MECHANICAL <4G69> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION
Item | Specification
--- | ---
Total displacement mL | 2,378
Bore × Stroke mm | 87 × 100
Compression ratio | 9.5
Compression chamber | Pentroof
Camshaft arrangement | SOHC
Number of valve | Intake | 8
Exhaust | 8
Valve timing | Intake valve | Open (BTDC) | 6° <low speed cam>
20° <High speed cam>
Closes (ABDC) | 38° <low speed cam>
72° <High speed cam>
Exhaust valve | Open (BTDC) | 60°
Closes (ABDC) | 16°
Fuel system | Electronically controlled multipoint fuel injection
Rocker arm | Roller type

[11E] ENGINE MECHANICAL <4G69> - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation