[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - DETONATION SENSOR - REMOVAL AND INSTALLATION <4G6-SOHC, 4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

DETONATION SENSOR

REMOVAL AND INSTALLATION <4G6-SOHC, 4G6-DOHC>
CAUTION Do not drop or hit the detonation sensor against other components. Internal damage may result, and the detonation sensor will need to be replaced.
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Detonation sensor connector connection
<<A>> | >>A<< | 2. | Detonation sensor
| REMOVAL SERVICE POINT
| <<A>> DETONATION SENSOR REMOVAL
| Use special tool detonation sensor wrench (MD998773) to remove the detonation sensor.
| INSTALLATION SERVICE POINT
| >>A<< DETONATION SENSOR INSTALLATION
| Use special tool detonation sensor wrench (MD998773) to tighten the detonation sensor to the specified torque.

[16] ENGINE ELECTRICAL - - IGNITION SYSTEM - DETONATION SENSOR - REMOVAL AND INSTALLATION <4G6-SOHC, 4G6-DOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation