[32] POWER PLANT MOUNT - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

GENERAL INFORMATION The inertia axial system has been adopted for the engine mounting system. Pressurized liquid-filled longitudinally installed cylindrical engine mounting is adopted to reduce vibration during acceleration and cornering. The liquid-filled transmission mounting improves riding comfort by its refined insulator. Installation of roll mounting in the upper area limits engine rolling. Further more, large diameter insulator reduces idle vibration. CONSTRUCTION DIAGRAM

[32] POWER PLANT MOUNT - - GENERAL INFORMATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation