[3] WELDED PANEL REPLACEMENT - - REAR END CROSSMEMBER | PRINT PAGE / INDEX / PRIOR / NEXT

REAR END CROSSMEMBER
| NOTE ON REPAIR WORK
| REMOVAL
| If the rear end crossmember outer comes in contact with the quarter inner extension lower, distance the welding points from the specifications of the figure (instructions) and leave a slight clearance, then pull forward the dotted line of the rear end crossmember outer.
| Turn the bottom portion of the rear end crossmember upward and remove, as shown in the figure of the instructions.

[3] WELDED PANEL REPLACEMENT - - REAR END CROSSMEMBER | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation