[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.21 Cancel Latch Signal System | PRINT PAGE / INDEX / PRIOR / NEXT

Code No.21 Cancel Latch Signal System
DIAGNOSIS CODE SET CONDITIONS The engine-A/T-ECU communicates cancellation retention information between the two microprocessors. This diagnosis code is set when cancellation retention information contains inconsistency.
PROBABLE CAUSE Malfunction of the engine-A/T-ECU.
| DIAGNOSIS Replace the engine-A/T-ECU (Refer to GROUP 13C, Engine-A/T-ECU ). Then check that diagnosis code 21 is not set.

[17] ENGINE AND EMISSION CONTROL - - AUTO-CRUISE CONTROL <4G69-VEHICLES WITH AUTO-CRUISE CONTROL SYSTEM> - DIAGNOSTIC TROUBLE CODE PROCEDURES - Code No.21 Cancel Latch Signal System | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation