[2] BODY DIMENSIONS - - TYPE A (PROJECTED DIMENSIONS) - UNDER BODY <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

TYPE A (PROJECTED DIMENSIONS)

UNDER BODY <2000> NOTE: The * mark indicates the mounting position for the frame centering gauge.
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
1* | Centre of under cover mounting hole | Round | 8
2 | Front sidemember inner notch | - | -
3* | Centre of crossmember mounting hole | Round | 18
4* | Centre of front floor sidemember positioning hole | Round | 25
5* | Centre of rear seat crossmember side water draining hole | Oblong | 38 × 22
6 | Centre of rear floor sidemember water draining hole | Round | 16
7* | Centre of towing hook mounting hole | Round | 15
8 | Tip of centre bearing mounting bolt (4WD) (left-front side) | - | -
9 | Tip of centre bearing mounting bolt (4WD) (right-front side) | - | -
10 | Tip of centre bearing mounting bolt(4WD) (left-rear side) | - | -
11 | Tip of centrebearing mounting bolt (4WD) (right-rear side) | - | -
NOTE: The assumed standard line is established 100 mm below the measurement point No.4.

[2] BODY DIMENSIONS - - TYPE A (PROJECTED DIMENSIONS) - UNDER BODY <2000> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation