[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION PROCEDURE FOR TROUBLE SYMPTOMS - INSPECTION PROCEDURE 4: Faulty ABS Operation | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 4: Faulty ABS Operation
TECHNICAL DESCRIPTION (COMMENT) The cause depends on driving and road surface conditions, so diagnosis may be difficult. However, if no diagnosis code is displayed, carry out the following inspection.
TROUBLESHOOTING HINTS (The most likely causes for this case:) Malfunction of the hydraulic unit
| DIAGNOSIS Check the hydraulic unit. (Refer to .) If the hydraulic unit (integrated with ABS-ECU) is malfunctioning, replace it. Then check that the malfunction symptom is eliminated.

[35B] ANTI-SKID BRAKING SYSTEM (ABS) - - TROUBLESHOOTING - INSPECTION PROCEDURE FOR TROUBLE SYMPTOMS - INSPECTION PROCEDURE 4: Faulty ABS Operation | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation