[54A] CHASSIS ELECTRICAL - - HEADLAMP - TROUBLESHOOTING - TROUBLESHOOTING <Vehicles with headlamp auto cut function> | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLESHOOTING

TROUBLESHOOTING <Vehicles with headlamp auto cut function>
Features the headlamp automatic shutdown function to avoid battery drain when the headlamps are left on. The main features are as follows: Extinguishes automatically in three minutes if the ignition switch is turned off with the lighting switch on. Extinguishes in one second if the driver's door is opened within that 3-minute period. If the headlamps are turned on with the ignition switch off, the headlamps and tail lamps will extinguish in three minutes after the driver's door is opened or closed. The headlamps are controlled by the Smart Wiring System (SWS). For troubleshooting, refer to respective Groups below. Using SWS monitor <Hong Kong spec.>: GROUP 54C, Trouble shooting . Not using SWS monitor <Except for Hong Kong spec.>: GROUP 54D, Trouble shooting .

[54A] CHASSIS ELECTRICAL - - HEADLAMP - TROUBLESHOOTING - TROUBLESHOOTING <Vehicles with headlamp auto cut function> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation