[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 11. POWER STEERING FLUID LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

| 11. POWER STEERING FLUID LEVEL
| Check that the fluid level is between "MAX" and "MIN". If the fluid is added, start the engine and turn the steering wheel from stop to stop several times to expel air from the system. Specified gear oil: Automatic transmission fluid DEXRON II

[1] PRE-DELIVERY INSPECTION - - UNDER HOOD - 11. POWER STEERING FLUID LEVEL | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation