[3] WELDED PANEL REPLACEMENT - - REAR FLOOR | PRINT PAGE / INDEX / PRIOR / NEXT

REAR FLOOR
NOTE: Refer to the Rear End Crossmember section on for the welding points with the rear end crossmember.
| NOTE ON REPAIR WORK
| REMOVAL
| When cutting the rear floor pan, cut it from 310 ± 100 mm behind the rear seat back assembling hole.
| INSTALLATION <2400>
| When assembling the rear floor sidemember extension (left side), insert it between the rear floor sidemember and rear floor sidemember reinforcement rear.

[3] WELDED PANEL REPLACEMENT - - REAR FLOOR | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation