[11B] ENGINE OVERHAUL <4G6-SOHC> - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

EXHAUST MANIFOLD

REMOVAL AND INSTALLATION
<4G63 ENGINE>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Engine hanger
| >>A<< | 2. | Water outlet fitting
|  | 3. | Engine hanger
|  | 4. | Exhaust manifold cover
|  | 5. | Oxygen sensor
|  | 6. | Exhaust manifold bracket
|  | 7. | Exhaust manifold
|  | 8. | Exhaust manifold gasket
<4G64 ENGINE>
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Engine hanger
| >>A<< | 2. | Water outlet fitting
|  | 3. | Engine hanger
|  | 4. | Exhaust manifold cover
|  | 5. | Exhaust manifold
|  | 6. | Exhaust manifold gasket
| INSTALLATION SERVICE POINTS
| >>A<< EXHAUST MANIFOLD BRACKET INSTALLATION
| Apply a 3 mm diameter bead of FIPG to the surface shown in the drawing. Specified sealant: Mitsubishi Genuine Part No.MD970389 or equivalent

[11B] ENGINE OVERHAUL <4G6-SOHC> - - EXHAUST MANIFOLD - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation