[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - UNDERDRIVE CLUTCH AND INPUT SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

UNDERDRIVE CLUTCH AND INPUT SHAFT

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
|  | 1. | Snap ring
|  | 2. | Input shaft
|  | 3. | Seal ring
| >>D<< | 4. | Snap ring
| >>C<< | 5. | Clutch reaction plate
| >>C<< | 6. | Clutch disc
| >>C<< | 7. | Clutch plate
<<A>> | >>B<< | 8. | Snap ring
|  | 9. | Spring retainer
| >>A<< | 10. | D-ring
|  | 11. | Return spring
|  | 12. | Underdrive clutch piston
| >>A<< | 13. | D-ring
| >>A<< | 14. | D-ring
|  | 15. | Underdrive clutch retainer
| DISASSEMBLY SERVICE POINTS
| <<A>> SNAP RING REMOVAL
| Use the special tools to remove the snap ring. Spring compressor (MD998907) Spring compressor retainer (MD998924)
| REASSEMBLY SERVICE POINTS
| >>A<< D-RING INSTALLATION
| Apply ATF, blue petrolatum jelly or white Vaseline to the D-rings and handle them carefully not to damage them during installation.
| >>B<< SNAP RING INSTALLATION
| Use the special tools to install the snap ring. Spring compressor (MD998907) Spring compressor retainer (MD998924)
| >>C<< CLUTCH PLATE/CLUTCH DISC/CLUTCH REACTION PLATE INSTALLATION
| CAUTION Soak the clutch discs in ATF before assembling it. Assemble the clutch plates, clutch discs, and clutch reaction plates with their non-toothed portions (A in the illustration) aligned with the hole (B in the illustration) formed in a crest of the underdrive clutch retainer.
| Orient the clutch reaction plate as shown in the illustration when it is installed.
| >>D<< SNAP RING INSTALLATION Install the snap ring. Press down the clutch reaction plate on its entire circumference using the special tools. Spring compressor (MB991628) Spring compressor retainer (MD998924)
| Check the clearance between the snap ring and clutch reaction plate. If the clearance is not within the standard value range, make adjustment by selecting a snap ring of an appropriate thickness. Standard value: 1.6 - 1.8 mm

[23B] AUTOMATIC TRANSMISSION OVERHAUL <F4A4/W4A4> - - UNDERDRIVE CLUTCH AND INPUT SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation