[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 24. OPERATION OF SERVICE BRAKES AND PARKING BRAKES | PRINT PAGE / INDEX / PRIOR / NEXT

| 24. OPERATION OF SERVICE BRAKES AND PARKING BRAKES
| Service brakes Turn up the carpet, etc under the brake pedal. Check the clearance between the brake pedal and the toeboard when the brake pedal is depressed. If the clearance does not meet the specifications, check for air in the system, brake fluid leakage, and/or a malfunction of the pedal itself. Clearance between the brake pedal and the toeboard: Standard value: 100 mm or more
| Verify correct brake pedal free play. NOTE: For inspection and adjustment of the brake pedal free play, refer to GROUP 2, Periodic Inspection and Maintenance. Parking brake Check the parking brake drag and lever travel. NOTE: For inspection of the parking brake lever, refer to GROUP 2, Periodic Inspection and Maintenance.

[1] PRE-DELIVERY INSPECTION - - BEFORE ROAD TEST - 24. OPERATION OF SERVICE BRAKES AND PARKING BRAKES | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation