[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLE SYMPTOM CHART
Symptom | Inspection procedure number | Reference page
--- | --- | ---
Communication with the MUT-II/III is not possible. | A-1 |
When the ignition switch is at the LOCK (OFF) position, the functions do not work normally. | A-2 |
Check the ETACS-ECU battery power supply circuit.
<FUNCTION SYSTEM>
Symptom | Inspection procedure number | Reference page
--- | --- | ---
Alarm Functions | Ignition key reminder buzzer function does not work. <Vehicles for GCC only> | B-1 |
Lamp reminder buzzer function does not work normally. | B-2 |
Central door locking | Central door locking system does not work. | LH drive vehicles | C-1 |
RH drive vehicles |
A door or a tailgate can not be locked or unlocked by the central door locking system. | LH drive vehicles | C-2 |
RH drive vehicles |
The central door locking system can not be operated by means of the front passenger's door key cylinder. | C-3 |
The ignition key reminder buzzer function does not work normally. | C-4 |
The impact detection door unlock function does not function. | C-5 |
Power window | Power windows do not work at all. | Except vehicles for Argentina | D-1 |
Vehicles for Argentina |
Driver's power window does not work by means of the power window main switch. | Except vehicles for Argentina | D-2 |
Vehicles for Argentina |
Relevant power window(s) do not work by means of the front and rear passenger's power window sub switches. | LH drive vehicles except for Argentina | D-3 |
LH drive vehicles for Argentina |
RH drive vehicles |
Front and/or rear passenger's power window(s) do not work by means of the power window main switch. | LH drive vehicles except for Argentina | D-4 |
LH drive vehicles for Argentina |
RH drive vehicles |
The power window timer function does not work normally. | Except vehicles for Argentina | D-5 |
Vehicles for Argentina |
The window glass lowers automatically while it is rising. | D-6 |
Power window anti-trap function does not work normally. <Vehicles for Argentina> | D-7 |
Keyless entry system | Keyless entry system does not work. | E-1 |
Keyless entry hazard warning lamp answerback function or the room lamp answerback function does not work normally. | E-2 |
Encrypted code cannot be registered. | E-3 |
The timer lock function does not work after the doors have been unlocked by the keyless entry system. | E-4 |
Sunroof | The sunroof does not work at all. | F-1 |
Any of the sunroof switch positions is defective. | F-2 |
Sunroof timer function does not work normally. | Except vehicles for Australia | F-3 |
Vehicles for Australia |
Sunroof anti-trap function does not work normally. | F-4 |
Windshield wiper and washer | The windshield wipers do not work at all. | G-1 |
The windshield wipers does not work when the wiper switch is at "INT", "WASHER" or "MIST" position. However, the wipers work at low speed when the switch is at "LO" and "HI" position. | G-2 |
The windshield wipers do not stop at the specified park position. | G-3 |
The windshield wipers does not work normally. | G-4 |
The intermittent wiper interval can not be adjusted by operating the windshield intermittent wiper volume control. | G-5 |
The intermittent wiper interval is not changed according to the vehicle speed. <Except vehicles for GCC> | G-6 |
The windshield washer does not work. | G-7 |
Rear wiper and washer | The rear wiper does not work at all. | H-1 |
The rear wiper does not stop at the specified park position. | H-2 |
When the selector lever is moved to "R" position during the rear wiper operation, the rear wiper does not operate at the continuous mode. | H-3 |
The rear washer does not work. | H-4 |
Headlamp washer | The headlamp washer does not work. | I-1 |
Ignition key cylinder illumination lamp | The ignition key cylinder illumination lamp does not illuminate/extinguish normally. | J-1 |
Seat belt warning lamp <Vehicles for Australia only> | The seat belt warning lamp does not flash normally. | K-1 |
Headlamp and tail lamp | The tail lamps do not illuminate normally. | L-1 |
The low-beam headlamps do not illuminate normally. | L-2 |
The high-beam headlamps do not illuminate normally. | L-3 |
The high-beam and low-beam headlamps do not illuminate when the passing switch is operated. | L-4 |
The headlamp automatic shutdown function does not work normally. <Except vehicles for Australia> | L-5 |
Any of tail lamps, position lamps or licence plate lamp does not illuminate. | L-6 |
The headlamp(s) do not illuminate. <including high-beam indicator> | L-7 |
Flasher timer | The turn-signal lamps do not illuminate. | M-1 |
The hazard warning lamps do not illuminate. | M-2 |
Any of the turn-signal lamps does not illuminate. | M-3 |
Fog lamp | The front fog lamps do not illuminate normally. | N-1 |
The rear fog lamps do not illuminate normally. <Vehicles for Argentina> | N-2 |
Any of the front fog lamps does not illuminate. | N-3 |
Any of the rear fog lamps does not illuminate. <Vehicles for Argentina> | N-4 |
Interior lamp | The front or rear room lamp does not illuminate or extinguish normally. <Vehicles without keyless entry system> | O-1 |
The front and rear room lamp does not illuminate or extinguish normally. <Vehicles with keyless entry system> | O-2 |
Interior lamp automatic shutoff function does not work normally. <Vehicles with keyless entry system> | O-3 |
The door-ajar warning lamp does not illuminate/extinguish normally. | O-4 |

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - TROUBLE SYMPTOM CHART | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation