[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - FOG LAMP - INSPECTION PROCEDURE N-1: The front fog lamps do not illuminate normally. | PRINT PAGE / INDEX / PRIOR / NEXT

FOG LAMP

INSPECTION PROCEDURE N-1: The front fog lamps do not illuminate normally.
| CAUTION Whenever the ECU is replaced, ensure that the input and output signal circuits are normal.
| OPERATION The ETACS-ECU operates this function in accordance with the input signals below. Tail lamp switch Headlamp switch Front fog lamp switch If the front fog lamps do not illuminate normally, these input signal circuit(s) or the ETACS-ECU may be defective.
| POSSIBLE CAUSES Malfunction of the column switch Malfunction of the front fog lamp switch Malfunction of the ETACS-ECU Damaged harness wires and connectors
| DIAGNOSIS PROCEDURE
| Step 1. Check that the tail lamps and headlamps operate. Check that the tail lamps and headlamps illuminate normally. Q: Is the check result normal? YES: Go to Step 2. NO: Check the tail lamps and the headlamps (Refer to trouble symptom chart ).
| Step 2. Pulse check Check the input signals below, which are related to the front fog lamps.
System switch | Check condition
--- | ---
Ignition switch (IG1) | When turned from ACC to ON
Tail lamp switch | When the lighting switch is turned to the TAIL position
Headlamp switch | When the lighting switch is turned to the HEADLAMP position
Front fog lamp switch | When the front fog lamp switch is turned from off to on
OK: The MUT-II/III sounds or the voltmeter needle fluctuates. Q: Is the check result normal? All the signals are received normally.: Go to Step 3. The ignition switch (IG1) signal is not received.: Refer to Inspection Procedure P-2 "The ignition switch (IG1) signal is not received ." The tail lamp switch signal is not received.: Refer to Inspection Procedure P-5 "The column switch (lighting and turn-signal lamp switch) signal is not received ." The headlamp switch signal is not received.: Refer to Inspection Procedure P-5 "The column switch (lighting and turn-signal lamp switch) signal is not received ." The front fog lamp switch signal is not received.: Refer to Inspection Procedure P-16 "The front fog lamp switch signal is not received ."
| Step 3. Connector check: A-05X front fog lamp relay connector Q: Is the check result normal? YES: Go to Step 4. NO: Repair the defective connector.
| Step 4. Check the front fog lamp relay. Refer to GROUP 54A - Front fog lamp . Q: Is the check result normal? YES: Go to Step 5. NO: Replace the front fog lamp relay.
| Step 5. Measure the voltage at the A-05X front fog lamp relay connector. Remove the front fog lamp relay, and measure at the relay box side. Check the voltage between the front fog lamp relay connector and body earth. Voltage between A-05X front fog lamp relay connector terminal No.1 and body earth Voltage between A-05X front fog lamp relay connector terminal No.2 and body earth OK: Battery positive voltage Q: Is the check result normal? YES: Go to Step 7. NO: Go to Step 6.
| Step 6. Check the wiring harness between A-05X front fog lamp relay connector (terminal Nos.1 and 2) and the battery. Check the power supply line for open circuit. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Repair the wiring harness.
| Step 7. Connector check: A-11X front-ECU connector Q: Is the check result normal? YES: Go to Step 8. NO: Repair the defective connector.
| Step 8. Check the wiring harness between A-05X front fog lamp relay connector terminal No.3 and A-11X front-ECU connector terminal No.11. Check the output lines for open circuit. Q: Is the check result normal? YES: Go to Step 9. NO: Repair the wiring harness.
| Step 9. Retest the system. Check that the front fog lamps illuminate normally. Q: Is the check result normal? YES: The trouble can be an intermittent malfunction (Refer to GROUP 00 - How to Cope with Intermittent Malfunction ). NO: Replace the ETACS-ECU.

[54D] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Except for Hong Kong spec.> - - SYMPTOM PROCEDURES - FOG LAMP - INSPECTION PROCEDURE N-1: The front fog lamps do not illuminate normally. | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation