[54A] CHASSIS ELECTRICAL - - ACCESSORY SOCKET - ACCESSORY SOCKET - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| ACCESSORY SOCKET RELAY CONTINUITY CHECK
Battery voltage | Tester connection | Specified condition
--- | --- | ---
Not applied | 1 - 4 | Open circuit
Connect terminal 2 to the positive battery terminal Connect terminal 3 to the negative battery terminal | 1 - 4 | Less than 2 ohms

[54A] CHASSIS ELECTRICAL - - ACCESSORY SOCKET - ACCESSORY SOCKET - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation