[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - PRIOR TO TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

TROUBLESHOOTING

| PRIOR TO TROUBLESHOOTING Before carrying out troubleshooting, check the following two items. Make sure that the ETACS-ECU, the junction block (J/B), the front-ECU and the engine compartment relay box are connected securely. Check that the system fuses and fusible links are not burned out.

[54B] SMART WIRING SYSTEM (SWS) NOT USING SWS MONITOR <Hong Kong spec.> - - TROUBLESHOOTING - PRIOR TO TROUBLESHOOTING | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation