[42] BODY - - DOOR - WINDOW GLASS RUNCHANNEL AND DOOR OPENING WEATHERSTRIP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

WINDOW GLASS RUNCHANNEL AND DOOR OPENING WEATHERSTRIP

REMOVAL AND INSTALLATION
|  |  | Waterproof film removal steps
--- | --- | --- | ---
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 1. | Pull handle bracket
|  | 2. | Waterproof film
|  |  | Door inner opening weatherstrip removal steps
|  | • | Cowl side trim (Refer to GROUP 52A, Trims ).
|  | 3. | Door inner opening weatherstrip (body side)
|  |  | Door outer opening weatherstrip removal steps
|  | • | Front door check mounting bolt (body side) (Refer to ).
<<A>> | >>C<< | 4. | Door outer opening weatherstrip
|  |  | Door beltline inner weatherstrip removal steps
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 5. | Door beltline inner weatherstrip
|  |  | Door window glass runchannel removal steps
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 1. | Pull handle bracket
|  | 2. | Waterproof film
|  | 5. | Door beltline inner weatherstrip
| >>B<< | 6. | Door window glass runchannel
|  |  | Door beltline moulding removal steps
|  | • | Door mirror assembly (Refer to GROUP 51, Door Mirror ).
|  | 7. | Door beltline moulding
DOUBLE-SIDED TAPE POSITION
|  |  | Waterproof film removal steps
--- | --- | --- | ---
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 1. | Pull handle bracket
|  | 2. | Waterproof film
|  |  | Door inner opening weatherstrip removal steps
|  | • | Rear seat (Refer to GROUP 52A, Trims ).
|  | • | Scuff plate (Refer to GROUP 52A, Trims ).
|  | 3. | Door inner opening weatherstrip (body side)
|  |  | Door outer opening weatherstrip removal steps
|  | • | Rear door check mounting bolt (body side) (Refer to ).
<<A>> | >>C<< | 4. | Door outer opening weatherstrip
|  |  | Door beltline inner weatherstrip removal steps
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 5. | Door beltline inner weatherstrip
|  |  | Door window glass runchannel removal steps
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
|  | 1. | Pull handle bracket
|  | 2. | Waterproof film
|  | 5. | Door beltline inner weatherstrip
|  | 6. | Door window glass runchannel
|  |  | Door beltline moulding removal
|  | 7. | Door beltline moulding
|  |  | Door tape removal steps
|  | • | Door trim assembly (Refer to GROUP 52A, Door Trim ).
| >>A<< | 8. | Door tape
DOUBLE-SIDED TAPE POSITION
| REMOVAL SERVICE POINT
| <<A>> DOOR OUTER OPENING WEATHERSTRIP REMOVAL
| Make a fabricated tool as shown in the illustration to remove the door weatherstrip.
| INSTALLATION SERVICE POINTS
| >>A<< DOOR TAPE <REAR DOOR> INSTALLATION
| Apply the door tape in the location shown in the Figure of the instructions.
| >>B<< DOOR WINDOW GLASS RUNCHANNEL <FRONT DOOR> INSTALLATION
| Assemble the run channel cut-out area with the thumb of the door mirror.
| >>C<< DOOR OUTER OPENING WEATHERSTRIP INSTALLATION The clip colour identifies the left and right weatherstrips so be sure to see the colours so as to install correctly.
APPLICABLE SIDE | IDENTIFICATION COLOUR
--- | ---
Left door | Natural (White)
Right door | Pink

[42] BODY - - DOOR - WINDOW GLASS RUNCHANNEL AND DOOR OPENING WEATHERSTRIP - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation