[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - Actuator Test Reference Table | PRINT PAGE / INDEX / PRIOR / NEXT

Actuator Test Reference Table
Item No. | Inspection item | Drive content | Inspection conditions | Normal condition | Code No. /Inspection procedure No. | Reference page
--- | --- | --- | --- | --- | --- | ---
01 | Injector | Cut off No. 1 injector | Engine: After warm-up, idle operation (Cut off injectors sequentially to check for a cylinder that does not change engine in idle status. | Engine is changed (becomes unstable or stalled) | Code No. P0201 |
02 | Cut off No. 2 injector | Code No. P0202 |
03 | Cut off No. 3 injector | Code No. P0203 |
04 | Cut off No. 4 injector | Code No. P0204 |
07 | Fuel pump | Drive fuel pump to circulate fuel | Ignition switch: "ON" | Check for pump operating noise near fuel tank | Operating noise audible | Procedure No. 25 |
08 | Purge control solenoid valve | Switch solenoid valve from OFF to ON | Ignition switch: "OFF" | When the valve is actuated, operating noise is audible | Code No. P0443 <Vehicles for Hong kong> |
17 | Basic ignition timing | Switch engine-A/T-ECU to ignition timing adjusting mode | Engine: Idle operation Install timing light | 5° BTDC | - | -
21 | Fan controller | Actuate fan motor | Ignition switch: "ON" A/C switch: ON | Fan motor is rotated | Procedure No. 22 |
22 | Oil control valve | Oil control valve turns from OFF the ON | Ignition switch: "ON" | Clicks when oil control valve is driven | Code No. P1021 <Vehicles for Hong kong> |
34 | Throttle valve control servo | Stop the throttle valve control servo | Ignition switch: "ON" | Throttle valve is open | Code No. P2100, P2101, P2102, P2103 |

[13C] MULTIPORT FUEL INJECTION (MPI) <4G69> - - TROUBLESHOOTING - Actuator Test Reference Table | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation