[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G63-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

STARTER MOTOR ASSEMBLY

REMOVAL AND INSTALLATION <4G63-SOHC>
Pre-removal and Post-installation Operation Resonator and Air Intake Duct Removal and Installation (Refer to GROUP 15, Air Cleaner ). Under Cover Removal and Installation (Refer to GROUP 51, Under Cover ).
|  |  | Removal steps
--- | --- | --- | ---
|  | 1. | Starter cover
|  | 2. | Starter connector
|  | • | Drive Belt (Refer to GROUP 11A, Crankshaft pulley ).
|  | • | A/C compressor connector
|  | • | A/C compressor connecting bolts
<<A>> |  | 3. | Starter assembly
|  | 4. | Starter cover bracket
| REMOVAL SERVICE POINT
| <<A>> STARTER ASSEMBLY REMOVAL
| Move the A/C compressor to one side to create sufficient clearance for the starter removal. Remove the starter assembly from underneath the vehicle.

[16] ENGINE ELECTRICAL - - STARTING SYSTEM - STARTER MOTOR ASSEMBLY - REMOVAL AND INSTALLATION <4G63-SOHC> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation