[37] POWER STEERING - - POWER STEERING GEAR BOX AND LINKAGE - TIE ROD END BALL JOINT DUST COVER REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| TIE ROD END BALL JOINT DUST COVER REPLACEMENT If the dust cover is damaged accidentally during service work, replace the dust cover as follows:
| Apply specified grease to the lip and inside of the dust cover. Specified grease: Multipurpose grease SAE J310, NLGI No.2 or equivalent Drive in the dust cover with special tool front axle base (MB990776) until it is fully seated. Check the dust cover for cracks or damage by pushing it with your finger.

[37] POWER STEERING - - POWER STEERING GEAR BOX AND LINKAGE - TIE ROD END BALL JOINT DUST COVER REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation