[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 34: Connector Lock System Detects Connector Unlocked | PRINT PAGE / INDEX / PRIOR / NEXT

Diagnosis code 34: Connector Lock System Detects Connector Unlocked
DIAGNOSIS CODE SET CONDITIONS This diagnosis code is set if a poor connection at the SRS-ECU is detected. However, if the vehicle condition returns to normal, diagnosis code number 34 will be automatically erased, and the SRS warning lamp will go out.
PROBABLE CAUSES Damaged connectors Malfunction of the SRS-ECU
| DIAGNOSIS PROCEDURE
| STEP 1. Connector check: SRS-ECU connector C-114 and C-115 Q: Are connectors correctly engaged? YES: Go to Step 2. NO: Engage the connectors correctly. Then go to Step 3.
| STEP 2. Connector check: SRS-ECU connector C-114 and C-115. Disconnect SRS-ECU connectors C-114 and C-115.
| Check the connector lock switch terminal inside the harness side connector for improper contact or deformation. Q: Are the SRS-ECU connector C-114 and C-115 in good condition? YES: Erase the diagnosis code memory, and check the diagnosis code. If diagnosis code 34 sets, replace the SRS-ECU (Refer to ). Then go to Step 3 . NO: Repair or replace the SRS-ECU connector C-114 and C-115. Then go to Step 3.
| STEP 3. Check whether the diagnosis code is reset. Q: Is diagnosis code 34 set? YES: There is no action to be taken. NO: The procedure is complete (If no malfunctions are found in all steps, an intermittent malfunction is suspected). Refer to GROUP 00 - How to Use Troubleshooting/Inspection Service Points .

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 34: Connector Lock System Detects Connector Unlocked | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation