[23A] AUTOMATIC TRANSMISSION (FF) - - A/T FLUID COOLER - REMOVAL AND INSTALLATION <4G64, 4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

A/T FLUID COOLER

REMOVAL AND INSTALLATION <4G64, 4G69>
Pre-removal and Post-installation Operation Front Under Cover (LH) Removal and Installation (Refer to GROUP 51, Under Cover .) A/T Fluid Supplying (Refer to .)
|  |  | Removal steps
--- | --- | --- | ---
<<A>> |  | • | Splash shield clip
|  | 1. | Cooler hose assembly
|  | 2. | A/T fluid cooler and bracket
|  | 3. | Bracket A
|  | 4. | Bracket B
|  | 5. | A/T fluid cooler
|  | 6. | Bush
|  | 7. | Collar
| REMOVAL SERVICE POINT
| <<A>> SPLASH SHIELD CLIP REMOVAL
| Remove the clip shown in the illustration.

[23A] AUTOMATIC TRANSMISSION (FF) - - A/T FLUID COOLER - REMOVAL AND INSTALLATION <4G64, 4G69> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation