[35A] BASIC BRAKE SYSTEM - - BRAKE PEDAL - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| STOPLIGHT SWITCH CHECK
| Connect an ohmmeter between the stoplight switch connector terminals. There should be no continuity between the terminals when the plunger is pushed in as shown. There should be continuity when it is released.

[35A] BASIC BRAKE SYSTEM - - BRAKE PEDAL - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation