[42] BODY - - DOOR - DOOR ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

DOOR ASSEMBLY

REMOVAL AND INSTALLATION
Post-installation Operation Door Fit Adjustment (Refer to .)
|  | Removal
--- | --- | ---
|  | 1. | Damper
|  | Door assembly removal steps
|  | • | Scuff Plate and Cowl Side Trim (Refer to GROUP 52A, Trims .)
|  | 2. | Harness connector
|  | 3. | Door check connecting bolt
|  | 4. | Door assembly
|  | 5. | Door upper hinge
|  | 6. | Door lower hinge
|  | Striker removal steps
| >>A<< | 7. | Striker
|  | 8. | Striker shim
|  | Door switch removal
|  | 9. | Door switch
| INSTALLATION SERVICE POINT
| >>A<< STRIKER INSTALLATION
| Align the centre of the striker and latch within ±1.5 mm, and install.

[42] BODY - - DOOR - DOOR ASSEMBLY - REMOVAL AND INSTALLATION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation