[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 46: Improper installation of SRS-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

Diagnosis code 46: Improper installation of SRS-ECU
| TROUBLE JUDGMENT The SRS-ECU monitors the passenger's airbag (squibs) voltage. The improper installation of SRS-ECU is detected if the SRS-ECU designed only for the driver's airbag is installed on the vehicle which has passenger's airbag, or if.the SRS-ECU designed for the passenger's airbag is installed on the vehicle which has driver's airbag only.
| POSSIBLE CAUSES Incorrectly installed SRS-ECU
| DIAGNOSIS Replace the SRS-ECU. (Refer to .)

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - TROUBLESHOOTING - DIAGNOSTIC TROUBLE CODE PROCEDURES - Diagnosis code 46: Improper installation of SRS-ECU | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation