[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B9. CHANGE GEAR OIL IN TRANSFER CASE (4WD) | PRINT PAGE / INDEX / PRIOR / NEXT

| B9. CHANGE GEAR OIL IN TRANSFER CASE (4WD)
| Remove oil filler plug and oil drain plug. Drain the gear oil.
| Before installing the plug, remove iron powder attached to the magnet of the drain plug. Tighten the oil drain plug to the specified torque. Tightening torque: 32 ± 2 N·m Fill the transfer case fresh oil by using a lubricator. Fill with specified oil till the level comes to the lower portion of oil filler plug hole. Specified transfer oil: Gear oil API classification GL-5 SAE 90 Quantity: 0.55 L Tighten the oil filler plug to the specified torque. Tightening torque: 32 ± 2 N·m

[2] PERIODIC INSPECTION AND MAINTENANCE - - OPERATIONS UNDER THE VEHICLE - B9. CHANGE GEAR OIL IN TRANSFER CASE (4WD) | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation