[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION Check the flow control valve of the pump body for clogging. Check the pulley and shaft for wear or damage. Check the rotor and vane groove for "stepped" wear. Check the contact surface of cam ring and vanes for "stepped" wear. Check the vanes for damage.

[37] POWER STEERING - - POWER STEERING OIL PUMP ASSEMBLY - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation