[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - THROTTLE POSITION SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

| THROTTLE POSITION SENSOR CHECK
| Disconnect the throttle position sensor connector. Measure the resistance between the throttle position sensor side connector terminal No. 1 and terminal No. 4. Standard value: 3.5 - 6.5 kΩ Measure the resistance between the throttle position sensor side connector terminal No. 2 and terminal No. 4.
Normal condition:
Throttle valve slowly open until fully open from the idle position | Changes smoothly in proportion to the opening angle of the throttle valve
| If the resistance is outside the standard value, or if it doesn't change smoothly, replace the throttle position sensor. NOTE: For the throttle position sensor adjustment procedure, refer to .

[13A] MULTIPORT FUEL INJECTION (MPI) <4G63> - - ON-VEHICLE SERVICE - THROTTLE POSITION SENSOR CHECK | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation