[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| WINDSHIELD WASHER MOTOR CHECK
| Remove the washer tank assembly with the washer hose attached. Then fill the washer tank with water. Check to see that the water is vigorously sprayed when connecting the positive battery terminal to terminal number 2 and terminal number 1 to the negative battery terminal.
| WINDSHIELD WASHER FLUID EJECTION CHECK Move the nozzle to adjust the position so that the spray is in the area shown in the illustration.
| WINDSHIELD WASHER SWITCH CHECK <L.H. DRIVE VEHICLE>
| Check continuity between the switch terminals.
Switch position | Tester connection | Specified condition
--- | --- | ---
OFF | 6 - 7 | Open circuit
Windshield washer switch | 6 - 7 | Less than 2 ohms
| <R.H. DRIVE VEHICLE> NOTE: The windshield washer switch is integrated in the column-ECU, so can not be checked as an individual part. However, its operation can be checked by the input signal check. Not using SWS monitor: Refer to GROUP 54B, Troubleshooting or GROUP 54D, Troubleshooting . Using SWS monitor: Refer to GROUP 54C, Troubleshooting or GROUP 54E, Troubleshooting .

[51] EXTERIOR - - WINDSHIELD WIPER AND WASHER - WINDSHIELD WASHER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation