[2] BODY DIMENSIONS - - TYPE A (PROJECTED DIMENSIONS) - SUSPENSION INSTALLATION DIMENSIONS <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

SUSPENSION INSTALLATION DIMENSIONS <2400>
No. | Standard measurement point | Hole shape | Size mm
--- | --- | --- | ---
3 | Centre of crossmember mounting hole | Round | 18
4 | Centre of front floor sidemember positioning hole | Round | 25
12 | Centre of front shock absorber mounting hole | Round | 110
13 | Centre of rear shock absorber mounting hole | Round | 64
14 | Tip of crossmember mounting bolt (left) | - | -
15 | Tip of crossmember mounting bolt (right) | - | -
16 | Centre of crossmember mounting hole | Round | 11
17 | Centre of trailing arm mounting hole | Round | 16
18 | Centre of trailing arm mounting hole | Round | 16
19 | Centre of crossmember mounting hole | Round | 28
20 | Centre of crossmember mounting hole | Round | 14
21 | Centre of crossmember mounting hole | Round | 13.5
22 | Centre of crossmember mounting hole | Round | 13.5
NOTE: The assumed standard line is established 100 mm below the measurement point No.4.

[2] BODY DIMENSIONS - - TYPE A (PROJECTED DIMENSIONS) - SUSPENSION INSTALLATION DIMENSIONS <2400> | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation