[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - DIFFERENTIAL CARRIER OIL SEAL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

| DIFFERENTIAL CARRIER OIL SEAL REPLACEMENT Remove the drive shaft from the differential carrier. (Refer to.) Remove the differential carrier oil seal.
| Use the following special tools to press-fit a new oil seal. Installer bar (MB990938) Oil seal installer (MB991115) Apply multi-purpose grease to the oil seal lip and drive shaft oil seal seating area. Replace the drive shaft circlip with a new one, and install the drive shaft to the differential carrier. (Refer to.)

[27B] REAR AXLE <4WD> - - ON-VEHICLE SERVICE - DIFFERENTIAL CARRIER OIL SEAL REPLACEMENT | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation