[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SEAT BELTS WITH PRE-TENSIONER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

| INSPECTION
| WARNING If any component damage is found during the following inspection, replace the seat belt with pre-tensioner with a new one. Dispose of the old one according to the specified procedure (Refer to ). Never attempt to measure the circuit resistance of the seat belt pre-tensioner even if you are using the specified tester. If the circuit resistance is measured with a tester, accidental seat belt pre-tensioner operation will result in serious personal injury. Check the pre-tensioner deployment section for dents and deformation. Check the harness and connector for damage and the terminals for deformation.

[52B] SUPPLEMENTAL RESTRAINT SYSTEM (SRS) - - SEAT BELTS WITH PRE-TENSIONER - INSPECTION | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation