[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 27: No Sound (CD only). | PRINT PAGE / INDEX / PRIOR / NEXT

INSPECTION PROCEDURE 27: No Sound (CD only).
DIAGNOSIS PROCEDURE
STEP 1. Check again using a normal CD, which is not dirty or scratched. Q: When you substitute another normal CD, is the CD played normally? YES: The original CD is defective. The CD player should sound normally. NO: Go to Step 2.
STEP 2. Check power supply to the CD player when the ignition switch is at "ACC" or "ACC". Q: Is the radio and CD player energized when the ignition switch is turned to the "ACC" or "ON position? YES: Replace the CD player. The procedure is complete. NO: Check the memory backup power supply circuit. Refer to Inspection Procedure 1 .

[54A] CHASSIS ELECTRICAL - - RADIO WITH TAPE PLAYER AND CD PLAYER - SYMPTOM PROCEDURES - INSPECTION PROCEDURE 27: No Sound (CD only). | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation