[37] POWER STEERING - - STEERING SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

DISASSEMBLY AND REASSEMBLY
|  |  | Disassembly steps
--- | --- | --- | ---
<<A>> | >>A<< | 1. | Special bolt
| >>A<< | 2. | Steering lock bracket
| >>A<< | 3. | Steering lock cylinder assembly
|  | 4. | Steering column shaft assembly
| DISASSEMBLY SERVICE POINT
| <<A>> SPECIAL BOLT REMOVAL
| Drill in the special bolt a hole deep enough for the tap to stand. Remove the special bolt with a left-hand tap.
| REASSEMBLY SERVICE POINT
| >>A<< STEERING LOCK CYLINDER ASSEMBLY/STEERING LOCK BRACKET/SPECIAL BOLT INSTALLATION CAUTION The steering lock bracket and bolts must be replaced with new ones when the steering lock is installed. When installing the steering lock cylinder assembly and steering lock bracket to the column tube, temporarily install the steering lock in alignment with the column boss.
| After checking that the lock works properly, tighten the special bolts until the head twists off.

[37] POWER STEERING - - STEERING SHAFT - DISASSEMBLY AND REASSEMBLY | PRINT PAGE / INDEX / PRIOR / NEXT

©2004 Mitsubishi Motors Corporation